{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet1 (2)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":2,"rows_kept":37,"cut":false,"hidden":true,"merged":[]}
[1,"赵依欣"]
[2,"华俊淇"]
[3,"董博"]
[4,"孙艳娇"]
[5,"郭静雨"]
[6,"李雨轩"]
[7,"曾庆绅"]
[8,"张珂娇"]
[9,"王永康"]
[10,"李紫涵"]
[11,"乔正秋"]
[12,"刘宏兴"]
[13,"姜海波"]
[14,"刘泰志"]
[15,"薛磊"]
[16,"穆含韵"]
[17,"穆穆"]
[18,"孙宜萱"]
[19,"王紫乔"]
[20,"翟坤"]
[21,"毕雨朵"]
[22,"陈亦博"]
[23,"梁博涵"]
[24,"马海珊"]
[25,"董睿颖"]
[26,"杨浩杰"]
[27,"杨明辉"]
[28,"李怡霏"]
[29,"王钰琪"]
[30,"杨云龙"]
[31,"李昱昊"]
[32,"韩佳欣"]
[33,"李贺豫"]
[34,"石小龙"]
[35,"魏怡然"]
[36,"赵海燕"]
[37,"吕建明"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Sheet1 (2)","index":2,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[[2,1,2,2],[2,3,2,4],[2,5,2,6],[4,1,4,6],[5,1,5,6],[24,1,24,6],[25,1,25,6],[26,1,26,2],[26,3,26,4],[26,5,26,6],[31,1,31,5],[32,1,32,2],[32,3,32,5],[51,1,51,5],[52,1,52,5],[0,0,1,8],[27,0,28,8],[54,0,55,6]]}
["烟熏炉主题参数和配置"]
[]
[" 型号","30型",null,"50型",null,"100型"]
["发烟方式","内置发烟","外置发烟","内置发烟","外置发烟","内置发烟","外置发烟"]
["电源","220/380V 50Hz"]
["控制方式","电脑板全自动"]
["安装尺寸","1300-1100-1700","2000-1100-1700","1400-1100-1900","2000-1100-1900","1500-1200-2200","2010-1200-2200"]
["箱体尺寸","1000-900-1350","1000-900-1350","1100-1100-1500","1100-1100-1500","1400-1200-1700","1400-1200-1700"]
["工作空间","720-870-890","720-870-940","820-950-1100","820-950-1100","1050-1200-1200","1050-1200-1200"]
["物料车尺寸","670-790-890","670-790-890","780-900-1050","780-900-1050","970-1040-1220","970-1040-1220"]
["产能","30kg/炉","30kg/炉","50kg/炉","50kg/炉","100kg/炉","100kg/炉"]
["小车数量",1,1,1,1,1,1]
["网盘数量",3,3,4,4,6,6]
["总功率","15kw","15kw","15kw","15kw","18kw","18kw"]
["设备材料","SUS304","SUS304","SUS304","SUS304","SUS304","SUS304"]
["风机功率","1.5kw","1.5kw","1.5kw","1.5kw","2.2kw","2.2kw"]
["风机转速","2800r/min","2800r/min","2800r/min","2800r/min","2800r/min","2800r/min"]
["风扇数量",1,1,1,1,1,1]
["叶轮材质","铝合金","铝合金","铝合金","铝合金","铝合金","铝合金"]
["叶轮直径","300mm","300mm","300mm","300mm","300mm","300mm"]
["叶轮数量",1,1,1,1,1,1]
["保温层厚度","50mm","50mm","50mm","50mm","50mm","50mm"]
["保温层材质","硅酸铝","硅酸铝","硅酸铝","硅酸铝","硅酸铝","硅酸铝"]
["最高工作温度","120℃","120℃","120℃","120℃","120℃","120℃"]
["高压蒸汽","≤0.2Mpa"]
["低压蒸汽","≤0.1Mpa"]
["报价",13500,null,18500,null,28500]
["烟熏炉主题参数和配置"]
[]
["型号","150型","250型","500型","750型","1000型"]
["发烟方式","外置发烟","外置发烟","外置发烟","外置发烟","外置发烟"]
["电源","380V 50Hz"]
["控制方式","电脑板全自动",null,"电脑板全自动/PLC全自动"]
["安装尺寸","2100-1250-2300","2200-1200-3000","2500-2400-3000","2500-3600-3000","2500-4800-3000"]
["箱体尺寸","1450-1250-1800","1480-1200-2530","1500-2400-2530","1500-3600-2530","1500-4800-2530"]
["工作空间","1050-1200-1500","1100-1100-2000","1100-2200-2000","1100-3300-2000","1100-4400-2000"]
["物料车尺寸","980-970-1560","1050-1050-1970","1050-1050-1970","1050-1050-1970","1050-1050-1970"]
["产能","150kg/炉","250kg/炉","500kg/炉","750kg/炉","1000kg/炉"]
["小车数量",1,1,2,3,4]
["网盘数量",6,"7～9","7～9","7～9","7～9"]
["总功率","24kw","27kw","48kw","68kw","90kw"]
["设备材料","SUS304","SUS304","SUS304","SUS304","SUS304"]
["风扇功率","3kw","4kw","4kw","4kw","4kw"]
["风扇转速","2800r/min","2800r/min","2800r/min","2800r/min","2800r/min"]
["风扇数量",1,1,2,3,4]
["叶轮材质","铝合金","铝合金","铝合金","铝合金","铝合金"]
["叶轮直径","320mm","400mm","400mm","400mm","400mm"]
["叶轮数量",1,1,2,3,4]
["保温层厚度","50mm","60mm","60mm","60mm","60mm"]
["保温层材质","硅酸铝","硅酸铝","硅酸铝","硅酸铝","硅酸铝"]
["最高工作温度","120℃","120℃","120℃","120℃","120℃"]
["高压蒸汽","≤0.2Mpa"]
["低压蒸汽","≤0.1Mpa"]
["报价","37500/34500","62000/58000","78000/73500","125000/12000","164000/155000"]
["联系厂家：山东，联系人：魏经理：13505369114"]